IR LED transmitter

20mm lens

35 mm lens

PIN photodiode receiver

Range depends on transmitter power

4 mA: 100 feet 14 mA: 183 feet preamp detector amp low-pass filter comparator

to microcontroller

0.9 mA total at 6 Vdc

6V (3 D cells)

John P. Beale 2/9/94

Infrared Link: Block Diagram